                ********************************************
                *                                          *
                *    Windows Printer Drivers Setup Disk    *
                *                                          *
                ********************************************

Thank you for purchasing our product.

You have just opened the README.TXT file. It contains
information about the installation of the printer driver that
comes with your package.

*** Very important: ***
 1. Please don't overwrite the files of "UNIDRV.DLL" and "ICONLIB.DLL" to your
    windows system while installing this driver.


Printer Driver Installation Guide:
==================================
There are 6 Windows platforms supported by the this driver disk.  Each driver
resides in different directory described as follows:

        Platform                        Directory
        --------                        ---------
        Windows 95                        WIN95
        Windows 98                        WIN98
        Windows 2000                      WIN2000
	Windows XP			  WinXP
	Windows 2003 Server		  Win2003
        Windows NT 4.0                    NT40


Installing Windows 95/98 Printer Driver:

 1.     Select the Settings entry from the Start menu.
 2.     Select the Printers entry from the Settings menu.
 3.     Double-click the "Add" Printer icon.
 4.     Click the "Next" button.
 5.     Select which port your printer is connected.
 6.     Click the "Next" button.
 7.     Click the "Have Disk" button.
 8.     Put the Driver Disk into the drive A: (or B:).
 9.     Click the "OK" button.
10.     Change directories to WIN95.
11.     Highlight the corresponding printer driver name.
12.     Click the "Next" button.
13.     Highlight the corresponding printer port.
14.     Click the "Configure Port" button if you need to configure your port
        settings.
15.     Click the "Next" button.
16.     Click the "Next" button.
17.     Choose "No" without printing a test page or
               "Yes" with printing a test page.
18.     Click the "Finish" button.


Installing Windows WIN2000/WINXP/NT 4.0 Printer Driver:

 1.     Select the Settings entry from the Start menu.
 2.     Select the Printers entry from the Settings menu.
 3.     Double-click the "Add" Printer icon.
 4.     Click the "Next" button.
 5.     Select which port your printer is connected.
 6.     Click the "Next" button.
 7.     Click the "Have Disk" button.
 8.     Put the Driver Disk into the drive A: (or B:).
 9.     Change directories to NT40.
10.     Click the "OK" button.
11.     Highlight the corresponding printer driver name.
12.     Click the "Next" button.
13.     Highlight the corresponding printer port.
14.     Click the "Configure Port" button if you need to configure your port
        settings.
15.     Click the "Next" button.
16.     Click the "Next" button.
17.     Choose "No" without printing a test page or
               "Yes" with printing a test page.
18.     Click the "Finish" button.


Release Notice:
===============
Ver 1.2.20
 1. In this version, we fixed the bug of control code for transferring to
    direct thermal mode of printer in Win95 platform.
 2. Add Win98 installation information file.
Ver 1.2.21
 1. In this version, we modified the limit of paper size to 8 inch for
    maximal width and 43 inch for maximal length in Win95, Win98 and
    NT operation system.
Ver 1.2.22
 1. In this version, we modified the environment parameters to avoid printing
    error in old NT 4.0 Germany version operation system.
 2. Add a sub-directory for installation of Traditional Chinese Windows version
    to avoid the UI page overlay between Traditional Chinese and English
    Windows version.
Ver 1.2.23
 1. Rename the develop identification code for mini-driver in Windows NT 4.0
    operation system.
Ver 1.2.24
 1. Add the utility to set some special parameters for PPLA printer language.
    Please read the readme file in "Utility" sub-directory for more
    installation information.
Ver 1.2.31
 1. Support Windows 2000 printer driver installation.
 2. Windows NT 3.51 and DOS commands generator will have not been included
    after this version.
 3. Separate printer driver into four models from original "Label Dr. 200".
Ver 1.2.41
 1. Modify the maximum printable label width to 168mm for 6 inch printer model.
 2. Modify printer driver to support bidirectional text printing, especially support the Arabic
    Windows version.
 3. Support Windows XP printer driver installation.
 4. Remove printer utility software from this driver disk. Please contact your vender for  
    support. 
Ver 1.3.00
 1. Add "Tear off" function in "Options" setting group of Windows printer driver.
 2. Add GDI commands to support new printers' modeles with centered paper guide. 
Ver 1.3.11    
 1. Support Windows XP printer driver installation.
Ver 1.3.12
 1. Add USB printer driver for Win 98, Win2000, WinXP.
 2. Add bi-direction communication for USB port.
Ver 1.3.13
 1. Support Windows 2003 Server printer driver installation.
 2. Add auto-install function.(only support for Win 98/2000/XP and 2003 Server)

TRADEMARKS
==========
All trademark or brand names mentioned are properties
of their respective companies.


============END==========
